The unit can be updated through a USB drive as follows.

1. Copy the updating file “MERGE.bin” to the root directory of the USB drive.
2. Connect the USB drive to the USB port on the rear of the device.

Attention: The USB port can only support maximum 500ma. Please use a small power U-disk as upgrading USB drive.

1. Connect a HDMI display to MS741/PS711.
2. Turn on MS741/PS711. The display device displays the HDMI output signal after normal boot of the device, as bellows:
3. Press and hold the INPUTS 1 button for more than five seconds, "System is upgrading…"is displayed in the display device, at the same time, all buttons indicators on the front panel blink, as bellows:

Attention: The unit can’t be power-off until the upgrading progress is finished. Or, the unit firmware will be corrupted.

1. After updating, “Upgrading is successful, system will reboot” is displayed in the display device. After seconds, the unit will reboot.
2. The unit reboots automatically.
3. Till now, the whole upgrading progress is finished.